110885 – Block Data Input Codes

Parking Lane or Other Special Lane:

* N – no parking lane and no other special lane
* PK – parking lane present on outside of traveled way or parking explicitly marked by pavement markings
* SP – parking is permitted on outside of traveled way but is not explicitly marked as a parking lane
* CLP – parking is permitted only for part of the day on the outside-most traveled lane (curb lane)
* BL – marked bicycle lane on roadway (sharrow markings alone do not constitute a bicycle lane; nor do off-road bicycle paths)
* OTH – other special lane present

Roadway Type:

* 2U – two-lane undivided
* 3T – two-lane with center two way left turn lane
* 4U – four-lane undivided
* 4D – four-lane divided
* 5T – four-lane with center two-way left turn lane
* 6U – six-lane undivided
* 6D – six-lane divided

Median Type:

* N – No median or median treatment (cross section with double yellow centerline)
* R – Raised median (separated from roadway by a curb)
* D – Depressed median (grass median with no curbs)
* F – Flush median (paved median flush with paved roadway surface)

Horizontal Alignment:

* T – Tangent
* GC – Gentle Curves
* SC – Sharp Curves

Shoulder Type:

* P – Paved shoulder
* T – Turf shoulder
* G – Gravel shoulder
* C – Composite shoulder
* VC – Vertical curb at edge of traveled way
* MC – Sloping or mountable curve at edge of traveled way
* CG – Vertical curb and gutter at edge of traveled way
* MG – Sloping or mountable curb and gutter at edge of traveled way
* PC - Paved shoulder with curb at outside edge of shoulder
* N – No shoulder (and no curb or curb and gutter)